{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":1,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":14,"n_cols":12,"rows_kept":14,"merged":[[0,0,2,8],[0,9,0,11],[1,9,1,11],[2,9,2,11],[3,0,3,1],[3,2,3,3],[3,4,3,5],[3,6,3,7],[3,8,3,11],[4,0,4,2],[4,3,4,11],[5,1,5,4],[5,5,5,8],[5,9,5,10],[6,1,6,4],[6,5,6,8],[6,9,6,10],[7,1,7,4],[7,5,7,8],[7,9,7,10],[8,1,8,4],[8,5,8,8],[8,9,8,10],[9,1,9,4],[9,5,9,8],[9,9,9,10],[10,1,10,4],[10,5,10,8],[10,9,10,10],[11,1,11,4],[11,5,11,8],[11,9,11,10],[12,1,12,4],[12,5,12,8],[12,9,12,10],[13,0,13,1],[13,2,13,3],[13,4,13,5],[13,6,13,7],[13,9,13,11]],"flags":["formulas_cached_only"]}
["    宁波三和壳体公司零部件检验指导书",{"$nulls":8}," 文件版本：A0"]
[{"$nulls":9}," 文件编号："]
[{"$nulls":9}," 修订日期：2010.7.06"]
["零件型号",null,"7278-2",null,"零件名称",null,"壳体",null,"样件   试生产   生产"]
["检验前准备工量具",null,null,"卡尺、色差仪、7278-1、7278-2、4974-5"]
["序号","检验项目和要求",{"$nulls":3},"图示",{"$nulls":3},"检验方法",null,"频率"]
[1,"零件材料",{"$nulls":3},"按订单要求",{"$nulls":5},"每批次"]
[2,"零件颜色",{"$nulls":3},"按订单要求",{"$nulls":3},"色差仪",null,"2小时"]
[3,"无明显缺陷：飞边、收缩、顶白、缺料、表面拉伤、变形",{"$nulls":3},"对比样品",{"$nulls":3},"目测",null,"2小时"]
[4,"与面框7278-1试装配是否良好",{"$nulls":7},"试装",null,"2小时"]
[5,"与安装架4974-5试装配是否良好",{"$nulls":7},"试装",null,"2小时"]
[6]
[7]
["编制/日期",null,"熊小花",null,"审核/日期",{"$nulls":3},"批准/日期"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}